A picture containing text, clipart

Description automatically generatedA picture containing text, clipart

Description automatically generated

Belt-Drive Bluetooth Turntable

A picture containing indoor, computer

Description automatically generated


331/3 and 45 rpm with Auto-Stop

Aluminium tone arm & platter

Audio Technica AT91 moving magnet cartridge

Built-In PHONO pre-amp

Anti-interference coupling circuit



A picture containing indoor, table

Description automatically generated

A picture containing text, indoor, electronics, computer

Description automatically generated

A picture containing indoor

Description automatically generated

SPECIFICATION

|  |  |
| --- | --- |
| Top Panel Controls | Speed Rotary Selector (331/3 rpm – 45 rpm)  Bluetooth Pairing Button |
| Rear Panel Controls | Slide Switch for Pre-amplifierOn/OFF selection for RCA jack output |
| Platter | Aluminum alloy |
| Tonearm | Aluminum alloy with anti-skate adjustment and adjustable counter-weight |
| Drive Transmission | Belt drive with auto rotation speed checking and correctionz-20KHz |
| Pick Up | Moving Magnetic Cartridge |
| Wireless Connectivity | Bluetooth A2DP wireless connection;  Bluetooth V5.1; Bluetooth Supports: HFP, A2DP, AVRCP profiles;  Bluetooth scope: 10meters or 33 feet |
| Analog Connectivity | RCA Left and Right |
| Equalization | Built-in RIAA equalizer |
| Power | AC110-220V,50/60HZ,13W |
| Origin | China |
| Accessories | AC power cord, spindle adaptor |
| Dimensions | (W x D x H) 440mm (175/16”) x 380mm (1415/16”) x 135mm (55/16”)  Box: 535mm (211/16”) x 456mm (1715/16”) x 190mm (71/2”) |
| Weight | 6.2kg (Gross box weight 6.9kg)  13lb 11oz (Gross box weight 15lb 4oz) |
| Barcode | EAN: 5060832950107  UPC: 860008515933 |
| SKU | 4020101 |
| Loading | 48×40” US (1219x1016mm) 1200x1000mm UK = 40 units  Euro Pallet = 36 units  20’ cntr 645 pcs, 40’ cntr 1290 |
| HS Tariff Code | 8519300000 |